
# description of the chip metadata
BLANK METADATA
  COMMENT  STR  MULTI
  COMMENT  STR
  COMMENT  STR  Basic Info about this frame
  COMMENT  STR
  SKYCELL  S32                       # Sky Cell ID number
  CELLVER  S32                       # Sky Cell version number
  FILTER   S32                       # Filter 
  STACKID  S32                       # ID for this image stack
  NP2IMGS  S32                       # Number of P2 images contributing
  ANALVER  S32                       # Software Analysis Version
  COMMENT  STR
  COMMENT  STR  Combination (P4S, P4D, Image Stack/ Cumulative Sky) Image
  COMMENT  STR  Metadata HDU
  COMMENT  STR  
  OBS_ID   STR  UnknownFormat       # Observation Identifier
  CLASSID  S32                    0 # Class ID = focal plane location
  DETECTID S32                    0 # Numerical ID of detector
  NX       S32                 4800 # Number of columns on the detector
  NY       S32                 4800 # Number of rows on the detector   DATE    STR 2006/02/05
  COMMENT  STR
  COMMENT  STR  Astrometric Solution (up to linear terms)
  COMMENT  STR
  NASTRO   S32                  100 # Number of astrometry stars
  CERROR   F32               10.000 # Scatter in astrometry solution (MAS)
  CTYPE1   STR  RA---TAN            # WCS Coordinate type
  CTYPE2   STR  DEC--TAN            # WCS Coordinate type
  CRVAL1   F32      321.30941666667 # WCS Ref value (RA in decimal degrees)
  CRVAL2   F32     -5.1685277777778 # WCS Ref value (DEC in decimal degrees)
  CRPIX1   F32    -1051.17692913657 # WCS Coordinate reference pixel
  CRPIX2   F32     2033.40939404705 # WCS Coordinate reference pixel
  CD1_1    F32  1.13378419402790E-4 # WCS Coordinate scale matrix
  CD1_2    F32  8.93919113249280E-8 # WCS Coordinate scale matrix
  CD2_1    F32  -5.4105516940550E-7 # WCS Coordinate scale matrix
  CD2_2    F32  -1.1365323690945E-4 # WCS Coordinate scale matrix
  COMMENT  STR
  COMMENT  STR  Higher order terms in astrometric solution
  COMMENT  STR
  POLYORD  S32                    3 # Polynomial Order
  PCA1X3Y0 F32                  0.0 # WCS, Axis 1, coefficient of X^3
  PCA1X2Y1 F32                  0.0 # WCS, Axis 1, coefficient of X^2 * Y
  PCA1X1Y2 F32                  0.0 # WCS, Axis 1, coefficient of X * Y^2
  PCA1X0Y3 F32                  0.0 # WCS, Axis 1, coefficient of Y^3
  PCA1X2Y0 F32                  0.0 # WCS, Axis 1, coefficient of X^2
  PCA1X1Y1 F32                  0.0 # WCS, Axis 1, coefficient of X * Y
  PCA1X0Y2 F32                  0.0 # WCS, Axis 1, coefficient of Y^2
  PCA1X3Y0 F32                  0.0 # WCS, Axis 2, coefficient of X^3
  PCA1X2Y1 F32                  0.0 # WCS, Axis 2, coefficient of X^2 * Y
  PCA1X1Y2 F32                  0.0 # WCS, Axis 2, coefficient of X * Y^2
  PCA1X0Y3 F32                  0.0 # WCS, Axis 2, coefficient of Y^3
  PCA1X2Y0 F32                  0.0 # WCS, Axis 2, coefficient of X^2
  PCA1X1Y1 F32                  0.0 # WCS, Axis 2, coefficient of X * Y
  PCA1X0Y2 F32                  0.0 # WCS, Axis 2, coefficient of Y^2
  COMMENT  STR
  COMMENT  STR  PSF Description Parameters
  COMMENT  STR
  PSFMOD   S32                    1 # PSF Model number
  PSFFWHM  F32                  1.0 # PSF Full width at Half Maximum (pixels)
  PSFWIDX  F32                  1.0 # PSF Width in X coordinate (pixels)
  PSFWIDY  F32                  1.0 # PSF Width in Y coordinate (pixels)
  PSFTHETA F32                  0.0 # PSF Orientation angle (degrees)
  PSF_EX1  F32                  0.0 # PSF Extra parameter #1
  PSF_EX2  F32                  0.0 # PSF Extra parameter #2
  COMMENT  STR
  COMMENT  STR  Photometry Calibration information
  COMMENT  STR
  COMMENT  STR   Formula for Photometry, based on keywords given in this header:
  COMMENT  STR   m = -2.5*log(DN) + 2.5*log(EXPTIME)
  COMMENT  STR   M = m + PHOT_C + PHOT_K*(AIRMASS - 1) + PHOT_X*(PHOT_C1 - PHOT_C2)
  COMMENT  STR
  PHOTCODE STR  GPC.00.r            # Photometry reduction code identifier
  PHOTOCID S32                      # Numerical code for reduction code
  PHOT_C   F32              25.7150 # Elixir zero point - measured for camera run
  PHOT_CS  F32               0.0048 # Elixir zero point - scatter
  PHOT_NS  S32                   19 # Elixir zero point - N stars
  PHOT_NM  S32                    5 # Elixir zero point - N images
  PHOT_C0  F32              25.7430 # Elixir zero point - nominal
  PHOT_X   F32               0.0830 # Elixir zero point - color term
  PHOT_K   F32              -0.0400 # Elixir zero point - airmass term
  PHOT_C1  STR  i_SDSS              # Elixir zero point - color 1
  PHOT_C2  STR  r_SDSS              # Elixir zero point - color 2
  COMMENT  STR
  COMMENT  STR  Some statistics on this image
  COMMENT  STR
  NDETECT  S32                 1000 # Number of detections
  MAGSAT   F32                15.0  # Magnitude at which sources saturate
  MAGCOMP  F32                22.0  # Magnitude for which frame is 95% complete
  SKYVAL   F32              1000.0  # Median sky value on detector
  SKYVAR   F32                 1.0  # Variance of sky values
  BIASVAL  F32               200.0  # Mean bias level of frame
  BIASVAR  F32                 1.0  # Variance of bias values
  COMMENT  STR
  COMMENT  STR  P2 images used to generate this image stack
  COMMENT  STR 
  COMMENT  STR
  COMMENT  STR  Quality Assurance Flags from IPP
  COMMENT  STR
  QAFLAGS  STR  UnknownValue        # IP QA flags
END

