||Name||Hexadecimal||Value||Description||
||DEFAULT||0x00000000||0||Initial value; resets all bits.||
||SECF_STAR_FEW||0x00000001||1||Used within relphot: skip star.||
||SECF_STAR_POOR||0x00000002||2||Used within relphot: skip star.||
||SECF_USE_SYNTH||0x00000004||4||Synthetic photometry used in average measurement.||
||SECF_USE_UBERCAL||0x00000008||8||Ubercal photometry used in average measurement.||
||SECF_HAS_PS1||0x00000010||16||PS1 photometry used in average measurement.||
||SECF_HAS_PS1_STACK||0x00000020||32||PS1 stack photometry exists.||
||SECF_HAS_TYCHO||0x00000040||64||Tycho photometry used for synthetic magnitudes.||
||SECF_FIX_SYNTH||0x00000080||128||Synthetic magnitudes repaired with zeropoint map.||
||SECF_RANK_0||0x00000100||256||Average magnitude calculated in 0th pass.||
||SECF_RANK_1||0x00000200||512||Average magnitude calculated in 1st pass.||
||SECF_RANK_2||0x00000400||1024||Average magnitude calculated in 2nd pass.||
||SECF_RANK_3||0x00000800||2048||Average magnitude calculated in 3rd pass.||
||SECF_RANK_4||0x00001000||4096||Average magnitude calculated in 4th pass.||
||SECF_STACK_PRIMARY||0x00004000||16384||PS1 stack photometry comes from primary skycell.||
||SECF_STACK_BESTDET||0x00008000||32768||PS1 stack best measurement is a detection (not forced).||
||SECF_STACK_PRIMDET||0x00010000||65536||PS1 stack primary measurement is a detection (not forced).||
||SECF_HAS_SDSS||0x00100000||1048576||This photcode has SDSS photometry.||
||SECF_HAS_HSC||0x00200000||2097152||This photcode has HSC photometry.||
||SECF_HAS_CFH||0x00400000||4194304||This photcode has CFH photometry (mostly megacam).||
||SECF_HAS_DES||0x00800000||8388608||This photcode has DES photometry.||
||SECF_OBJ_EXT||0x01000000||16777216||Extended in this band.||
